Supporting Information


**Brush-structured Sulfur-Polyaniline-Graphene composite as Cathodes for Lithium Sulfur Batteries**

Heguang Liua, Ruixuan Jinga, Caiyin Youa, Qifeng Zhong\*b

aSchool of Materials Science and Engineering, Xi’an University of Technology, Xi’an, 710048, China

bDepartment of Pharmaceutical Equipment and Electronic Instruments, School of Engineering, China Pharmaceutical University, Nanjing 210009, China

**Table S1**. The EIS simulation parameters of S-PANI-G before and after 100 cycles discharge charge treatment.



**Figure S1**. The equivalent circuit that was used to fit the experimental data.

