|  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **N°** | **Tool type** | **Length (mm)** | **Width (mm)** | **Thickness (mm)** | **Nb of UA** | **Motion** | **Location UA** | **Retouched edge** | **Edge angle** | **Worked material** | **Impact damages** | **Sharpening** |
| **952** | microblade | 8 | 4 | 1 | 1 | scrape | left | no | 35 | semi-hard | no | no |
| **10105** | microblade | 8,5 | 5 | 1,5 | 1 | cut/saw | left | no | \_ | butchery? | no | no |
| **2238b** | microblade | 9,5 | 6 | 2 | 1 | cut/saw | left | no | \_ | soft abrasive | no | no |
| **9045** | microblade | 9,5 | 4 | 1 | 1 | cut/saw | left | no | \_ | soft abrasive | no | no |
| **7704** | microblade | 9 | 5,5 | 1 | 1 | impact | the whole artifact | no | \_ | \_ | burin-like spin-off fracture 2mm long and lateral scars | no |
| **9548** | microblade | 10 | 6,5 | 1,5 | 1 | cut/saw | left | no | \_ | soft abrasive | no | no |
| **9083** | microblade | 14 | 5,5 | 1,5 | 1 | cut/saw | left | no | \_ | semi-hard abrasive | no | no |
| **9015** | microblade | 10 | 7 | 2 | 1 | cut/saw | right | no | \_ | soft abrasive | no | no |
| **9598** | microblade | 8 | 5 | 1,5 | 1 | scrape | left | no | 35 | semi-hard | no | no |
| **9082** | microblade | 5,5 | 4 | 1,5 | 1 | undet. | left | no | \_ | undet. | no | no |
| **9124** | microblade | 15 | 5,5 | 1,5 | 1 | cut/saw | left | no | 40 | butchery or hide ? | no | no |
| **9081** | microblade | 7,5 | 6 | 1,5 | 1 | cut/saw | left | no | \_ | butchery | no | no |
| **21834** | microblade | 19 | 5 | 2 | 1 | impact? | the whole artifact | no | \_ | \_ | burin-like spin-off fracture 3,5mm long | no |
| **21835** | microblade | 17 | 4 | 1,5 | 1 | impact? | the whole artifact | no | \_ | \_ | burin-like spin-off fracture 5,5mm long | no |
| **21959** | microblade | 10 | 5 | 1 | 2? | scrape + cut/saw? | left | no | 40 | dry hide ? | no | no |
| **21607** | microblade | 10 | 5 | 1 | 1 | impact? | the whole artifact | no | \_ | \_ | facial spin-off fracture 2,7mm long | no |
| **21927** | microblade | 8 | 5,5 | 1,5 | 1 | cut/saw | right | no | \_ | dry hide ? | no | no |
| **21531** | microblade | 17 | 4 | 2 | 1 | cut/saw | left | no | \_ | dry hide ? | undet. | no |
| **21557** | microblade | 12 | 5 | 1,5 | 1 | cut/saw | right | no | 35 | dry hide ? | no | no |
| **22088** | microblade | 11 | 4,5 | 1 | 2? | scrape + cut/saw? | left | no | 40 | semi-hard | no | no |
| **21877** | microblade | 8,5 | 5 | 1 | 1 | cut/saw | left | no | 42 | semi-hard | no | no |
| **21819** | microblade | 8,5 | 5,5 | 2 | 1 | cut/saw | right | no | \_ | soft abrasive | undet. | no |
| **21773** | microblade | 10,5 | 4 | 1,5 | 2? | scrape + cut/saw? | left | no | \_ | semi-hard abrasive | undet. | no |
| **21726** | microblade | 15,5 | 5 | 1,5 | 1? | cut/saw | left | yes | 25 | semi-hard | no | no |
| **21936a** | microblade | 6,5 | 5 | 1,5 | 2? | scrape + cut/saw? | left | no | 60 | soft abrasive | no | no |
| **21936b** | microblade | 7,5 | 5 | 1 | 1 | scrape | left | no | 40 | semi-hard abrasive | no | no |
| **21816a** | microblade | 6 | 4 | 1 | 1 | cut/saw | left | no | 42 | soft abrasive | no | no |
| **21816b** | microblade | 4,5 | 5 | 1,5 | 1 | scrape | left | no | 45 | semi-hard | no | no |
| **15899a** | microblade | 8 | 3 | 0,8 | 1 | cut/saw | left | no | 35 | butchery | no | no |
| **15974a** | microblade | 7,5 | 4,5 | 1,5 | 1 | cut/saw | left | no | 40 | semi-hard | no | no |
| **17513** | microblade | 10 | 4 | 1,5 | 1 | scrape | left | no | 40 | semi-hard | no | no |
| **15513** | microblade | 9,5 | 4 | 1 | 1 | impact | the whole artifact | no | \_ | \_ | burin-like spin-off fracture 3,5mm long and lateral scar | no |
| **10100** | microblade | 15,5 | 7 | 2 | 1 | scrape | left | no | 35 | semi-hard | no | no |
| **8495** | microblade | 6 | 4 | 1 | 1 | impact? | the whole artifact | no | \_ | \_ | lateral scars | no |
| **9463** | microblade | 15,5 | 5,5 | 1,5 | 1 | cut/saw | left | no | 35 | dry hide | no | no |
| **9468** | microblade | 18 | 5 | 1,8 | 1 | cut/saw | left | no | 35 | butchery? | no | no |
| **12942** | microblade | 10 | 5 | 1,5 | 1 | scrape | left | no | 35 | semi-hard | no | no |
| **13560** | microblade | 14,5 | 5 | 2 | 1 | cut/saw | left | no | \_ | semi-hard abrasive | no | no |
| **12700** | microblade | 7 | 5 | 1,7 | 1 | undet. | left | no | 40 | undet. | no | no |
| **8003** | microblade | 13 | 4,5 | 1,2 | 1 | cut/saw | left | no | 40 | butchery? | no | no |
| **8087** | microblade | 13,5 | 5,5 | 2 | 1 | cut/saw | right | no | 30 | dry hide | no | no |
| **8086** | microblade | 16,5 | 5 | 1,8 | 1 | cut/saw | left | no | 35 | soft abrasive | no | no |
| **8494** | microblade | 8 | 4 | 1,2 | 1? | undet. | left | no | 30 | soft | no | no |
| **8529** | microblade | 11,5 | 4 | 1,5 | 1 | scrape | left | no | 30 | semi-hard | no | no |
| **8461** | microblade | 10,5 | 5 | 1 | 1 | scrape | left | no | 45 | semi-hard | no | no |
| **8484** | microblade | 9 | 4,5 | 1,7 | 1 | cut/saw | left | no | 35 | semi-hard | no | no |
| **8119** | microblade | 9 | 5 | 1,1 | 2? | scrape + cut/saw? | left | no | 40 | semi-hard | no | no |
| **8154** | microblade | 7 | 4,5 | 1,1 | 1 | cut/saw | left | no | 35 | butchery? | no | no |
| **8096** | microblade | 8,5 | 4,5 | 1,1 | 1 | scrape | left | no | 30 | semi-hard | no | no |
| **9454** | microblade | 7 | 3,5 | 1,2 | 2 | scrape + cut/saw | left | no | \_ | undet. | no | no |
| **20052** | microblade | 9,5 | 4,5 | 1,5 | 1 | cut/saw | left | no | 35 | semi-hard abrasive | no | no |
| **20373** | microblade | 9 | 5 | 1 | 1 | cut/saw | left | no | 40 | butchery? | no | no |
| **20115** | microblade | 7,5 | 4,5 | 1,1 | 1 | cut/saw | left | no | \_ | soft abrasive | no | no |
| **20170** | microblade | 7,5 | 5 | 1,1 | 1 | cut/saw | left | no | \_ | soft abrasive | no | no |
| **20256** | microblade | 9 | 5 | 1,1 | 1 | cut/saw | left | no | \_ | soft abrasive | no | no |
| **8016** | microblade (backed) | 9,5 | 5 | 1,5 | 1 | cut/saw | left | yes | 40 | soft abrasive | no | undet. |
| **9500** | microblade (backed) | 9,5 | 4,5 | 1,3 | 1 | scrape | left | no | 35 | semi-hard abrasive | no | undet. |
| **21796** | microblade-like flake | 17,5 | 10 | 1,5 | 1 | incise | distal right (fracture corner) | no | 20 | semi-hard abrasive | no | no |
| **15724** | tool fragment | 6 | 15,5 | 3,5 | 1? | scrape | retouched edge | yes | 60 | semi-hard abrasive | no | undet. |
| **22740** | end scraper | 34 | 33 | 7,5 | 1 | scrape | distal | yes | 60 | dry hide | no | yes |
| **7993** | burin-scraper | 30 | 45 | 13,5 | 1 | scrape | right | yes | 45 | hard slightly abrasive | no | no |
| **26473** | burin spall | 32,5 | 7,5 | 4 | 1 | scrape | burin facet | yes | 85 | hard | no | yes |
| **26521** | burin spall | 15,5 | 5 | 2 | 1 | scrape | burin facet | yes | 50 | hard abrasive | no | yes |
| **15878** | burin spall | 21,5 | 4,5 | 3 | 1 | scrape | burin facet | yes | 85 | soft abrasive | no | yes |
| **20638** | burin spall | 17,5 | 5 | 5,5 | 1 | scrape | burin facet | yes | \_ | hard abrasive | no | yes |
| **13505** | burin spall | 25,5 | 7,5 | 9 | 1 | cut/saw | lateral edge | no | 50 | semi-hard abrasive | no | yes |
| **8504** | burin spall | 35,5 | 9,5 | 7,5 | 1 | scrape | burin facet | yes | 90 | hard slightly abrasive | no | yes |
| **8460** | burin spall | 37,5 | 3,5 | 7,5 | 1 | scrape | lateral edge | no | 45 | soft abrasive | no | yes |
| **21965** | burin spall | 46 | 11 | 8,5 | 1 | scrape | burin facet | yes | 75 | hard | no | yes |
| **12713** | burin spall | 34 | 11 | 5,5 | 1 | scrape | burin facet | yes | 70 | hard | no | yes |
| **15940** | burin | 38 | 43 | 7 | 1 | scrape | burin facet | yes | 85 | hard | no | yes |
| **19394** | burin | 26 | 36 | 14,5 | 5 | scrape | burin facets + flake unretouched edges | \_ | 70 to 100 | hard to semi-hard abrasive | no | yes |
| **13506** | burin | 33 | 26,5 | 5,5 | 1 | scrape | burin facet | yes | 60 | semi-hard abrasive | no | yes |
| **805** | burin | 43 | 31 | 5,5 | 1? | scrape | burin facet | yes | \_ | hard | no | yes |
| **21998** | burin | 37,5 | 32 | 10,5 | 1 | scrape | burin facet | yes | 80 | hard | no | yes |
| **20847** | blade-like flake | 20,5 | 17 | 4 | 1 | undet. | left | no | \_ | hard | no | yes |
| **12110** | bifacial shaping flake | 45 | 35,5 | 5,5 | 1 | cut/saw | distal right | no | 25 | soft | no | no |
| **15900** | bifacial preform fragment | 9,5 | 10 | 5,5 | 1? | scrape | left (biface edge) | yes | 60 |  | no | no |
| **20678** | bifacial preform fragment | 82,5 | 42 | 15 | 1 | dig ? | distal (biface tip) | yes | \_ | soft mineral | no | yes? |
| **21973** | bifacial preform fragment | 43,5 | 32,5 | 12,5 | 2 | cut/saw | right (biface edge) | yes | 40 | soft or semi-hard | no | undet. |
| **19752** | biface fragment | 52 | 23,5 | 9,5 | 2 | percussion | extremities (biface) | yes | \_ | hard | no | no |