Table S1: Carbon percentage in pottery samples determined using an elemental analyzer (EA) used in automated graphitization equipment (AGE) for combustion of samples

|  |  |  |  |
| --- | --- | --- | --- |
| S. No. | Sample Name | Carbon % before ABA treatment | Carbon % after ABA treatment |
| 1. | BGIc8 | 1.92 | 1.26 |
| 2. | BGIc9 | 2.09 | 1.24 |
| 3. | MRKc16 | 1.87 | 0.57 |
| 4. | SKGc3 | 1.65 | 1.15 |
| 5. | SLGc6 | 1.77 | 0.99 |