Movie 1
Case with inflow vapor concentration Υνapor,in = 0.9 and contact angle θ = 15°. 
Movie 2
Case with inflow vapor concentration Υνapor,in = 0.5 and contact angle θ = 15°. 
Movie 3
Case with inflow vapor concentration Υνapor,in= 0.1 and contact angle θ = 15°. 
Movie 4
Case with inflow vapor concentration Υνapor,in = 0.1 and contact angle θ = 30°. 
Movie 5
Case with inflow vapor concentration Υνapor,in = 0.1 and contact angle θ = 60°. 
Movie 6
Case with inflow vapor concentration Υνapor,in= 0.1 and contact angle θ = 105°.