Movie 1
Mode II oscillations of the flexible splitter with L/D =5.  In the case shown, EI = 5.45 x 10-06Nm, Re =11,263, K* = 1.63 X 10-5.
Movie 2
Mode I oscillations of the flexible splitter plate with L/D = 5.  In the case shown, EI = 7.50 x 10-04, Re = 14000, K* = 1.4 x 10-03.
Movie 3
Mode A oscillations of the flexible splitter plate with L/D = 2.  In the case shown, EI = 2.70 x 10-05 Nm, Re =20268, K * = 3.87 x -04.
Movie 4
Mode B oscillations of the flexible splitter plate with L/D = 2. In the case shown, EI = 2.70 x 10-05 Nm, Re = 7572, K * = 2.78 x 10-03.
Movie 5
Mode C oscillations of the flexible splitter plate with L/D = 2. In the case shown, EI = 7.50 x 10-04 Nm, Re = 5234, K * =1.6 x 10-01.
Movie 6
Mode D oscillations of the flexible splitter plate with L/D = 2. In the case shown, EI = 1.25 x 10-02 Nm, Re = 13557, K * =4.01 x 10-01.