# SUPPLEMENTARY MATERIAL

# ANTARCTIC SUBGLACIAL DRILLING RIG:PART II. IBED ICE AND BEDROCK ELECTROMECHANICAL DRILL

Pavel Talalay1, Xingchen Li1, Nan Zhang1\*, Xiaopeng Fan1, Youhong Sun1,2, Pinlu Cao1, Rusheng Wang1, Yang Yang1, Yongwen Liu1, Yunchen Liu1, Wei Wu1, Cheng Yang1, Jialin Hong1, Da Gong1, Han Zhang1, Xiao Li1, Yunwang Chen1, An Liu1, Yazhou Li1

1*Polar Research Center, Jilin University, Changchun, China*

2*China University of Geosciences, Beijing*

\*Correspondence to: znan@jlu.edu.cn

**Table S1**. Main results of ice drilling tests

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Run** | **Drilling fluid** | **Pump** | **Cutter type** | **Cutting load (N)** | **ROP (m h-1)** | **Penetration depth (mm)** | **Core catcher** | **Core length****(mm)** |
| 1 | Silicon oil | SPK4-11/11 | CSkB | <800 | 4.60 | 856 | + | 840 |
| 2 | Silicon oil | SPK4-11/11 | CSkB | <600 | 6.53 | 553 | + | 540 |
| 3 | Silicon oil | SPK4-11/11 | CSkB | <800 | 10.56 | 833 | + | 780 |
| 4 | Silicon oil | SPK4-11/11 | CSkB | <500 | 4.81 | 812 | + | 790 |
| 5 | Silicon oil | SPK4-11/11 | CSkB | <500 | 2.40 | 614 | + | 580 |
| 6 | Silicon oil | SPK4-11/11 | SC | <500 | 10.27 | 810 | + | 770 |
| 7 | Silicon oil | SPK4-11/11 | SC | <400 | 7.38 | 835 | + | 790 |
| 8 | Jet A-1 | SPK4-11/11 | SC | <400 | 7.50 | 835 | + | 795 |
| 9 | Jet A-1 | SPK4-11/11 | CStB | <400 | 6.67 | 839 | + | 835 |
| 10 | Jet A-1 | SPK4-11/11 | CStB | <800 | 4.02 | 708 | + | 700 |
| 11 | Jet A-1 | SPK4-11/11 | CStB | <800 | 2.70 | 775 | + | 745 |
| 12 | Jet A-1 | SPK4-11/11 | SC | <700 | 2.36 | 835 | + | 829 |
| 13 | Silicon oil | SPK4-11/11 | SC | <400 | 6.81 | 759 | + | 750 |
| 14 | Jet A-1 | SPK2-23/23 | SC | <500 | 7.95 | 855 | + | 810 |
| 15 | Jet A-1 | SPK2-23/23 | SC | <700 | 5.27 | 765 | + | 735 |
| 16 | Jet A-1 | SPK2-23/23 | SC | <400 | 6.69 | 861 | + | 830 |
| 17 | Jet A-1 | SPK2-23/23 | SC | <400 | 6.75 | 707 | + | 680 |
| 18 | Jet A-1 | SPK2-23/23 | SC | <300 | 4.37 | 560 | + | 550 |
| 19 | Jet A-1 | SPK2-23/23 | SC | <250 | 6.85 | 866 | + | 810 |
| 20 | Jet A-1 | SPK2-23/23 | SC | <250 | 6.76 | 853 | + | 800 |
| 21 | Jet A-1 | SPK2-23/23 | SC | <400 | 6.30 | 875 | + | 860 |
| 22 | Jet A-1 | SPK2-23/23 | SC | <400 | 6.80 | 858 | + | 845 |
| 23 | Jet A-1 | SPK2-23/23 | SC | <500 | 6.49 | 873 | + | 840 |
| 24 | Jet A-1 | SPK2-23/23 | SC | <400 | 6.91 | 864 | + | 830 |
| 25 | Exxsol D60 | SPK2-23/23 | SC | 800 | 5.26 | 2250 | + | 2187 |
| 26 | Exxsol D60 | SPK2-23/23 | SC | 800 | 7.60 | 2260 | + | 2221 |
| 27 | Exxsol D60 | SPK2-23/23 | SC | 800 | 8.75 | 2190 | + | 2159 |
| 28 | Exxsol D60 | SPK2-23/23 | SC | 900 | 7.42 | 2550 | + | 2521 |

\*CSkB – cutters with skewed blades; CStB – cutters with straight blades; SC – staggered cutters

**Table S2.** Main results of debris-containing ice drilling tests

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Run** | **Drill bit\*** | **Volume percentage of granite chips (%)** | **Average cutting load (N)** | **Average ROP (m h-1)** | **Penetration depth (mm)** |
| 1 | A | 10 | 1010 | 4.0 | 284 |
| 2 | B | 10 | 524 | 4.0 | 510 |
| 3 | A | 30 | 1063 | 1.9 | 364 |
| 4 | B | 30 | 1237 | 4.7 | 184 |
| 5 | C | 10 | 1131 | 1.6 | 118 |
| 6 | A | 30 | 1085 | 2.6 | 382 |
| 7 | B | 30 | 1074 | 10.9 | 692 |
| 8 | B | 10 | 1017 | 6.7 | 390 |

\* A – drill bit equipped by flat cutters with rake angle 0°; B – drill bit equipped by flat cutters with rake angle -10°; C – drill bit equipped by waved cutters with rake angle 0°

**Table S3.** Main results of bedrock drilling

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Run** | **Drilling fluid** | **Pump** | **Core barrel** | **Drill bit ID/OD (mm)** | **Cutting load (N)** | **ROP (m h-1)** | **Penetration (mm)** |
| 1 | Jet A-1 | SPK4-11/11 | Double-tube | 41/60 | <2000 | 0.74 | 700 |
| 2 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | <2000 | 1.1 | 720 |
| 3 | Jet A-1 | SPK2-23/23 | Double-tube | 41/60 | 1000-2000 | 0.85 | 539 |
| 4 | Jet A-1 | SPK2-23/23 | Single-tube | 41/60 | <2000 | 1.3 | 662 |
| 5 | Jet A-1 | SPK2-23/23 | Double-tube | 41/60 | 1500-2000 | 0.92 | 459 |
| 6 | Jet A-1 | SPK4-11/11 | Double-tube | 41/60 | <2000 | 0.9 | 523 |
| 7 | Jet A-1 | SPK4-11/11 | Double-tube | 41/60 | 1400-1700 | 0.75 | 652 |
| 8 | Jet A-1 | SPK4-11/11 | Double-tube | 41/60 | 1600-1800 | 0.7 | 612 |
| 9 | Jet A-1 | SPK4-11/11 | Double-tube | 41/60 | 1400-1600 | 0.73 | 468 |
| 10 | Silicon oil | SPK4-11/11 | Double-tube | 41/60 | <1000 | 0.39 | 117 |
| 11 | Silicon oil | SPK4-11/11 | Double-tube | 41/60 | 800-1000 | 0.2 | 49 |
| 12 | Silicon oil | SPK4-11/11 | Single-tube | 41/60 | 500-600 | 0.46 | 117 |
| 13 | Silicon oil | SPK4-11/11 | Single-tube | 41/60 | 500-600 | 0.45 | 87 |
| 14 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | <2000 | 0.45 | 523 |
| 15 | Silicon oil | SPK4-11/11 | Single-tube | 41/60 | 600-700 | 0.35 | 332 |
| 16 | Silicon oil | SPK4\_11-11 | Single-tube | 41/60 | 700-800 | 0.4 | 400 |
| 17 | Silicon oil | SPK4-11/11 | Single-tube | 41/60 | 800-900 | 0.57 | 50 |
| 18 | Silicon oil | SPK4-11/11 | Single-tube | 41/60 | 850-950 | 0.60 | 87 |
| 19 | Silicon oil | SPK4-11/11 | Single-tube | 41/60 | 800-950 | 0.35 | 100 |
| 20 | Silicon oil | SPK4-11/11 | Single-tube | 41/60 | 850-900 | 0.65 | 210 |
| 21 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～800 | 0.86 | 500 |
| 22 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～850 | 1.1 | 550 |
| 23 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1000 | 0.8 | 400 |
| 24 | Jet-A1 | SPK4-11/11 | Single-tube | 41/60 | ～1000 | 0.85 | 350 |
| 25 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1000 | 0.86 | 402 |
| 26 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1100 | 0.88 | 398 |
| 27 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1100 | 1.0 | 374 |
| 28 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1100 | 0.93 | 311 |
| 29 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～800 | 1.0 | 210 |
| 30 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～900 | 1.0 | 200 |
| 31 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1100 | 1.0 | 450 |
| 32 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1100 | 1.1 | 650 |
| 33 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1100 | 1.0 | 400 |
| 34 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1100 | 1.1 | 540 |
| 35 | Jet A-1 | SPK4-11/11 | Double-tube | 41/60 | ～1100 | 0.84 | 220 |
| 36 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1100 | 1.1 | 682 |
| 37 | Jet A-1 | SPK4-11/11 | Single-tube | 41/60 | ～1100 | 1.1 | 650 |
| 38 | Jet A-1 | SPK4-11/11 | Double-tube | 41/60 | ～1200 | 0.86 | 383 |
| 39 | Jet A-1 | SPK4-11/11 | Double-tube | 41/60 | ～1100 | 0.85 | 652 |
| 40 | Jet A-1 | SPK4-11/11 | Double-tube | 41/60 | ～1100 | 0.76 | 203 |
| 41 | Jet A-1 | SPK4-11/11 | Single-tube | 41/61 | -1200 | 0.74 | 250 |
| 42 | Jet A-1 | SPK4-11/11 | Single-tube | 41/61 | -1200 | 0.7 | 200 |
| 43 | Jet A-1 | SPK4-11/11 | Single-tube | 41/61 | -1200 | 0.5 | 260 |
| 44 | Jet A-1 | SPK4-11/11 | Single-tube | 41/61 | 1100-1200 | 1.0 | 650 |
| 45 | Jet A-1 | SPK4-11/11 | Double-tube | 34/62 | 1150-1250 | 1.0 | 670 |
| 46 | Jet A-1 | SPK4-11/11 | Double-tube | 34/62 | 1150-1250 | 0.8 | 300 |
| 47 | Jet A-1 | SPK4-11/11 | Double-tube | 34/61 | 1150-1250 | 1.0 | 700 |
| 48 | Jet A-1 | SPK4-11/11 | Double-tube | 34/61 | 1100-1300 | 0.9 | 670 |