**Supporting information**

**High performance coaxial wire-shaped supercapacitors using ionogel electrolyte toward sustainable energy system**

Yongchao Liu1, Mugilan Narayanasamy1, Cheng Yang2, Minjie Shi\*,1,

Wei Xie5, Hanzhao Wu1, Chao Yan\*,1, Hua Hou,4 and Zhanhu Guo3, 6 \*

*1. School of Materials Science and Engineering, Jiangsu University of Science and Technology, Zhenjiang, 212003, China*

*2. State Key Laboratory for Metallic Matrix Composite Materials, School of Materials Science and Engineering, Shanghai Jiao Tong University, Shanghai 200240, China*

*3Integrated Composites Laboraotry (ICL), Department of Chemical and Biomolecular Engineering, University of Tennessee, Knoxville, TN 37996, USA*

*4College of Materials Science and Engineering, North University of China, Taiyuan, 030051, China*

*5 Key Laboratory of Lightweight and Reliability Technology for Engineering Vehicle, Education Department, Changsha University of Science & Technology, Changsha, China*

*6 Key Laboratory of Materials Processing and Mold (Zhengzhou University), Ministry of Education, National Engineering Research Center for Advanced Polymer Processing Technology, Zhengzhou University, Zhengzhou, China*

*\* Corresponding author:*

Email: chaoyan@just.edu.cn (C. Yan); shiminjie@ just.edu.cn (M. Shi); zguo10@utk.edu (Z. Guo)



Fig. S1 TEM image of porous carbon dodecahedrons.



Fig. S2 Tensile stress-strain curve of coaxial WSSCs.



Fig. S3 Self-discharging performance of coaxial WSSCs.